* Visualisatie van site
* Fix IP op de server
* Vlan aamaken
* Switch instellen
* Instellen access point

***Router:***

***Creating a Vlan*** :

Enable

conf t

int Gig0/0

VLAN 10

Exit

int Gig0/1

VLAN 20

Exit

Show vlan brief

***Assinging vlan :***

Conf t

Int Gig0/0

Switchport access vlan 10

Switchport mode access

Exit

Int Gig0/1

Switchport access vlan 20

Switchport mode access

Exit